**WAI-6510 Virtual serial port driver installation method**

* **When the computer needs to use the virtual serial port, the virtual serial port driver file needs to be installed. This driver is suitable for WINDOW XP and WINDOW 7, WINDOW 10 system comes with virtual serial port driver, no need to install this driver**

## Installation

## Install virtual serial port driver



Win32-setup is window7 32bit

Win64-setup is window7 64bit

Winxp-setup is windowxp

**Double click to install**

Window10 don’t need to Install virtual serial port driver


## Steps:

1.Connect the scanner to the computer and turn on the button


2.Switch the scanner to virtual serial communication mode, switch method: scan the setting code below

|  |  |
| --- | --- |
|  | **1** |
|  | **2** |
|  | **3** |


3.Right click on the computer and select properties




4.Unknown devices will appear in the device manager, as shown in the below picture



5.Right-click on the unknown device and select Update Driver Software in the pop-up optional box




6.In the page that pops up, select Browse computer to find driver software




7.Select the driver folder for the product：The driver for WAI-6510


Then click next step



8.If the Windows security prompt pops up when installing the driver, choose to always install this driver software



9.Wait for the driver to install successfully



10.After the driver is completed, the corresponding device port will appear in the device manager

